SIMISA@@@@@@@@@@JINX0D0t______


Wagon ( cd_363001_hk
	Comment ( verze: 8.10.2006 definice svetel MSTS Bin )
	Comment ( svetla upravil Robo )
        Comment ( Verze: 1.1 )
        Comment ( Datum: 28/3/2007 )
        Comment ( Uprava vykonove charakteristiky - plocha do 60 kmh dle skutecnosti )
        Comment ( Mez adhese: 188kN )
        Comment ( Antislip odstranen )        
        Comment ( Vykon nastaven pro stridavou cast = 3060 kW )
        Comment (** kveten 2018 - Igor Hnizdo - upravy pro ORTS. Vzhledem k samostatnym ozvucenim zde nastaveny parametry pro stridavy system. **)
        Comment (** cervenec 2018 - Igor Hnizdo - doplneni zapisu pro funkci ARR - pro toto je nutne mit stazenou neverejnou "pre-alpha" verzi
                  ORTS, ve ktere je kod ARR (automaticka regulace rychlosti) doplnen. V jinych verzich ORTS nemusi ENG fungovat a muze zpusobit 
                  nepredvidatelne chyby!!! Proto si puvodni ENG vzdy zalohujte!!! **)
	Comment (** autor kodu ARR: Jindrich Machalinek **)
	Comment (** prosinec 2018 - Igor Hnizdo - aktualizace brzd, nastaveni hlavniho vypinace a ARR **)

	Type ( Engine )
	WagonShape ( "cd_363001_hk.s" )
        Freightanim ( cd_363001fg_hk.s 1 1 )
        Size ( 3.00m 4.69m 16.856m )
	Mass ( 87t )
	WheelRadius ( 0.607m )
	InertiaTensor ( Box (3.00m 4.69m 16.856m) )

comment (** sprahla **)

	comment (** sprahlo zadni **)
	Coupling (
		Type ( Chain )
		Spring (
			Break ( 450kN 850kN )
			r0 ( 0cm 10cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	comment (** sprahlo predni **)
	Coupling (
		Type ( Chain )
		Spring (
			Break ( 450kN 850kN )
			r0 ( 0cm 10cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)

comment (** adheze **)
	ORTSAdhesion (
        ORTSCurtius_Kniffler ( 7.5 44 0.161 0.7 )
        ORTSSlipWarningThreshold ( 60 )
        )

	DerailRailHeight ( 4cm )
	DerailRailForce ( 307.5kN )
	DerailBufferForce ( 300kN )

comment (** pocet naprav - vypocet adheze pro brzdeni **)
	NumWheels ( 4 )
	
comment (** jizdni odpor - treni, vaha87t, rychlost 120km/h, celni plocha 10.5m2 **)
	Friction (
		1070.5N/m/s    -0.10    1.3mph    11.172N/m/s    1.859
		5.1N/rad/s	1	-1rad/s	0N/rad/s	1
	)
	
comment (** odpor v oblouku **)

	ORTSTrackGauge ( 1435mm )
	comment (** rozvor podvozku **)
	ORTSRigidWheelbase ( 3200mm )
	ORTSUnbalancedSuperelevation ( 152.4mm )
	
Comment (** Sberace - "delay" udava dobu zdvihani sberace, jelikoz simulator nedokaze identifikovat delku trvani animace sberace **)

ORTSPantographs (
          Pantograph (
                Delay ( 2s )
                )
          Pantograph (
                Delay ( 2s )
                )
        )


comment (** brzdovy system - ladeno do rezimu P, brzdy postupne odbrzditelne **)
comment (** brzdici vaha rezim P = 44t, brzdici procento = 51, zabrzdna draha dle nomogramu 804m ze 100km/h **)
comment (** brzdici vaha rezim G = 24t, brzdici procento = 27, zabrzdna draha dle nomogramu 900m z 80km/h **)

  	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake" )
	BrakeSystemType( "Air_single_pipe" )
	comment (** rezim P - 109.2kN **)
	comment (** rezim G se lisi pouze dobou plneni valcu, MaxBrakeForce tedy v principu zustava stejna **)
	MaxBrakeForce( 109.2kN )
	MaxHandbrakeForce( 6kN )
	NumberOfHandbrakeLeverSteps( 10 )

	TripleValveRatio( 2.33 )
	comment (** rezim P = 0.15625bar/s - odbrzdeni 22.4s **)
	comment (** rezim G = 0.07bar/s - odbrzdeni 50s **)
	MaxReleaseRate( 0.15625bar/s )
	comment (** rezim P = 0.660bar/s - zabrzdeni 5.3s **)
	comment (** rezim G = 0.159bar/s - zabrzdeni 22s **)
	MaxApplicationRate( 0.660bar/s )
	EmergencyResCapacity( 150l )
	EmergencyResVolumeMultiplier ( 1 )
	EmergencyBrakeResMaxPressure( 5bar )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 3.5bar )
  comment (** objem brzdoveho potrubi **)
	BrakePipeVolume ( 14l )

	Comment (** Prubeh soucinitele treni dle rychlosti - litinove brzdove spalky - autor: Pajavlaky **)
ORTSBrakeShoeFriction (
  	

		       0.0	0.3100
		       1.0	0.2800
		       2.0	0.2670
		       3.0	0.2572
		       4.0	0.2490
		       5.0	0.2419
		       6.0	0.2355
		       7.0	0.2296
		       8.0	0.2242
		       9.0	0.2192
		       10.0	0.2145
		       11.0	0.2100
		       12.0	0.2059
		       13.0	0.2019
		       14.0	0.1981
		       15.0	0.1945
		       16.0	0.1911
		       17.0	0.1878
		       18.0	0.1847
		       19.0	0.1817
		       20.0	0.1788
		       21.0	0.1760
		       22.0	0.1733
		       23.0	0.1708
		       24.0	0.1683
		       25.0	0.1660
		       26.0	0.1637
		       27.0	0.1615
		       28.0	0.1594
		       29.0	0.1574
		       31.0	0.1536
		       32.0	0.1518
		       33.0	0.1501
		       34.0	0.1484
		       35.0	0.1468
		       37.0	0.1439
		       38.0	0.1425
		       40.0	0.1399
		       41.0	0.1387
		       51.0	0.1277
		       57.0	0.1217
		       63.0	0.1163
		       68.0	0.1123
		       74.0	0.1080
		       80.0	0.1044
		       87.0	0.1009
		       94.0	0.0982
		       105.0	0.0949
		       120.0	0.0919
		       140.0	0.0897
		       160.0	0.0897

                      )



comment (** pohled "cestujiciho" - z leveho okna kabiny **)

Inside (
		PassengerCabinFile ( 363001.s )
		PassengerCabinHeadPos ( -1.65 3.0 6.6 )
		RotationLimit ( 40 90 0 )
		StartDirection ( 0 -20 0 )
	)


  comment (** Svetla - CD, 2 dalkove/tlumene reflektory, oddelena bila/cervena pozicni svetla, upravil Igor Hnizdo **)
	Lights ( 41
		Light (
			comment (** Svetelny kuzel dalkovy tma **)
			Type ( 1 )
			Conditions (
			Unit ( 2 )
			Headlight ( 3 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( AAEED15D )
			  	Position ( 0.0 2.585 7.91 )
					Angle ( 17 )
					Transition ( 1 )
					Radius ( 190 )
				)
			)
		)
		Light (
			comment (** Svetelny kuzel tlumeny tma **)
			Type ( 1 )
			Conditions (
			Unit ( 2 )
			Headlight ( 2 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( 0.0 2.585 7.91 )
					Angle ( 20 )
					Transition ( 1 )
					Radius ( 65 )
				)
			)
		)
		Light (
			comment (** Svetelny kuzel dalkovy zkraceny - svetlo **)
			Type ( 1 )
			Conditions (
			Unit ( 2 )
			Headlight ( 3 )
			TimeOfDay ( 1 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( AAEED15D )
			  	Position ( 0.0 2.585 7.91 )
					Angle ( 16 )
					Transition ( 1 )
					Radius ( 85 )
				)
			)
		)
		
		comment (** Predni stanoviste **)

		Light (
			comment ( reflektor dalkovy levy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( -0.1 2.585 7.91 )
					Azimuth ( 0 0 0 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( reflektor dalkovy pravy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.11 2.585 7.91 )
					Azimuth ( 0 0 0 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( reflektor tlumeny levy )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( -0.1 2.585 7.91 )
					Azimuth ( 0 0 0 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor tlumeny pravy )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.11 2.585 7.91 )
					Azimuth ( 0 0 0 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Predni leve pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.74 1.66 7.83 )
					Azimuth ( 0 0 0 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Predni prave pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
       				 Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.74 1.66 7.83 )
					Azimuth ( 0 0 0 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( predni leve zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( -0.74 1.66 7.83 )
					Azimuth ( 0 0 0 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( predni prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( C0EED15D )
					Position ( 0.74 1.66 7.83 )
					Azimuth ( 0 0 0 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni leve pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
        			Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.74 1.66 -7.83 )
					Azimuth ( 180 180 180 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni prave pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
        			Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.74 1.66 -7.83 )
					Azimuth ( 180 180 180 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni leve koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.98 1.66 -7.83 )
					Azimuth ( 180 180 180 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni prave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.98 1.66 -7.83 )
					Azimuth ( 180 180 180 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		
		comment (** Zadni stanoviste **)

		Light (
			comment ( reflektor dalkovy levy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( -0.1 2.585 -7.91 )
					Azimuth ( 180 180 180 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( reflektor dalkovy pravy )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.1 2.585 -7.91 )
					Azimuth ( 180 180 180 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( reflektor tlumeny levy )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( -0.1 2.585 -7.91 )
					Azimuth ( 180 180 180 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor tlumeny pravy )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 2 )
			FadeOut ( 2 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.1 2.585 -7.91 )
					Azimuth ( 180 180 180 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Predni leve pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( -0.74 1.66 -7.83 )
					Azimuth ( 180 180 180 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( Predni prave pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( 0.74 1.66 -7.83 )
					Azimuth ( 180 180 180 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( predni leve zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( -0.74 1.66 -7.83 )
					Azimuth ( 180 180 180 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( predni prave zapnute )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( C0EED15D )
					Position ( 0.74 1.66 -7.83 )
					Azimuth ( 180 180 180 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni leve pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( -0.74 1.66 7.83 )
					Azimuth ( 0 0 0 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni prave pozicni )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( 0.74 1.66 7.83 )
					Azimuth ( 0 0 0 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni leve koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FF0000 )
					Position ( -0.98 1.66 7.83 )
					Azimuth ( 0 0 0 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( zadni prave koncove )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FF0000 )
					Position ( 0.98 1.66 7.83 )
					Azimuth ( 0 0 0 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		comment (** Loose consist **)

		Light	(
			comment( Prave predni pozicni - LC )
			Type ( 0 )
			Conditions (
			Unit ( 2 )
			Control ( 1 )
			Service ( 1 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( 0.74 1.66 7.83 )
					Azimuth ( 0 0 0 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light	(
			comment( Leve zadni pozicni - LC )
			Type ( 0 )
			Conditions (
			Unit ( 3 )
			Control ( 1 )
			Service ( 1 )
			TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 60EED15D )
					Position ( -0.98 1.66 -7.83 )
					Azimuth ( 180 180 180 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)

		comment (** Traffic (TR) - loko ovladana PC - smer vpred **)

		Light (
			comment ( TR predni prave )
			Type ( 0 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( 0.74 1.66 7.83 )
					Azimuth ( 0 0 0 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( TR predni leve )
			Type ( 0 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( -0.74 1.66 7.83 )
					Azimuth ( 0 0 0 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.7 )
				)
			)
		)
		Light (
			comment ( TR reflektor predni 1 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( -0.1 2.585 7.91 )
					Azimuth ( 0 0 0 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( TR reflektor predni 2 )
			Conditions (
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.11 2.585 7.91 )
					Azimuth ( 0 0 0 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC zadni leve koncove )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FF0000 )
					Position ( -0.98 1.66 -7.83 )
					Azimuth ( 180 180 180 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC zadni prave koncove )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FF0000 )
					Position ( 0.98 1.66 -7.83 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Elevation ( 10 10 10 )
					Radius ( 0.5 )
				)
			)
		)
		
		comment (** Traffic (TR) - loko ovladana PC - smer vzad **)

		Light (
			comment ( TR predni prave )
			Type ( 0 )
			Conditions (
				Unit ( 5 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( 0.74 1.66 -7.83 )
					Azimuth ( 180 180 180 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( TR predni leve )
			Type ( 0 )
			Conditions (
				Unit ( 5 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 60EED15D )
					Position ( -0.74 1.66 -7.83 )
					Azimuth ( 180 180 180 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( TR reflektor predni 1 )
			Conditions (
				Unit ( 5 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( -0.1 2.585 -7.91 )
					Azimuth ( 180 180 180 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( TR reflektor predni 2 )
			Conditions (
				Unit ( 5 )
				Control ( 1 )
				Service ( 2 )
				TimeOfDay ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.1 2.585 -7.91 )
					Azimuth ( 180 180 180 )
					Elevation ( -10 -10 -10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC zadni leve koncove )
			Type ( 0 )
			Conditions (
				Unit ( 4 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FF0000 )
					Position ( -0.98 1.66 7.83 )
					Azimuth ( 0 0 0 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( PC zadni prave koncove )
			Type ( 0 )
			Conditions (
				Unit ( 4 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 80FF0000 )
					Position ( 0.98 1.66 7.83 )
					Azimuth ( 0 0 0 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.5 )
				)
			)
		)
	)

 comment (** vnejsi zvuk **)
	Sound ( "..\\..\\common.snd\\sndX6X\\363eng-IH-OR.sms" )
)

Engine ( cd_363001_hk

	Wagon ( cd_363001_hk )

	Type ( Electric )
	comment (** nastaveno pro stridave napajeni 25kV/50Hz **)
	MaxPower ( 3060kW )
	MaxForce ( 296.48kN )
	MaxContinuousForce ( 176.1kN )
	MaxVelocity ( 120km/h )
	DieselEngineSpeedOfMaxTractiveEffort ( 66.4km/h )
	MaxCurrent ( 1100A )
	WheelRadius ( 0.607m )
	Sanding ( 30km/h )
	MaxSandingTime ( 600 )
	comment (** adhezni vaha - u stroje se vsemi dvojkolimi hnacimi (zde Bo'-Bo') je shodna s hmotou stroje **)
	ORTSDriveWheelWeight ( 87t )
	
comment (** Hlavni vypinac **)

        ORTSCircuitBreaker ( Manual )
        ORTSCircuitBreakerClosingDelay ( 0.22s )
        ORTSPowerOnDelay ( 1.0s )
        ORTSAuxPowerOnDelay ( 18s )
        
comment (** ARR - je potreba mit stazenou pre-alpha verzi 0.6 ORTS, ktera ma ARR (zatim ve vyvoji) implementovano **)

        ORTSCruiseControl (
		Equipped ( True )
		MaxForceSteps ( 12 )
		DynamicBrakeMaxForceAtSelectorStep ( 7 )
		DynamicBrakeDescentCoefficient ( 0.5 )
		AntiWheelSpinEquipped ( True )
		NominalSpeedStep ( 5 )
		UseThrottle ( False )
		Options ( "RegulatorManual, RegulatorAuto, RegulatorTest, SelectorParking, SelectorNeutral, SelectorOn, SelectorStart" )
	)

        
comment (** Tabulka trakcnich charakteristik pro radu 363 - autor: Paashi **)
    	
	ORTSTractionCharacteristics (   141   13
   throttle (      0   0.27   0.36   0.45   0.55   0.62   0.65   0.73   0.77   0.82   0.91   1.00   )
   table (                                          
      0km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      1km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      2km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      3km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      4km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      5km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      6km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      7km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      8km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      9km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      10km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      11km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      12km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      13km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      14km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      15km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN
      16km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      17km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      18km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      19km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      20km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      21km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      22km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      23km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.35kN   
      24km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.55kN   223.64kN   239.77kN   271.97kN   294.59kN   
      25km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   179.37kN   210.79kN   223.83kN   239.94kN   271.97kN   292.83kN   
      26km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   179.76kN   211.03kN   224.01kN   240.11kN   271.97kN   291.07kN   
      27km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.92kN   180.14kN   211.26kN   224.20kN   240.27kN   271.97kN   289.31kN   
      28km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.78kN   168.32kN   180.51kN   211.50kN   224.38kN   240.44kN   271.97kN   287.55kN   
      29km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.98kN   168.71kN   180.88kN   211.73kN   224.57kN   240.60kN   271.97kN   285.78kN   
      30km/h   0.00kN   52.88kN   80.65kN   111.84kN   144.18kN   169.10kN   181.25kN   211.96kN   224.75kN   240.76kN   271.97kN   284.30kN   
      31km/h   0.00kN   52.88kN   80.65kN   111.96kN   144.38kN   169.48kN   181.61kN   212.19kN   224.93kN   240.92kN   271.97kN   282.49kN   
      32km/h   0.00kN   52.88kN   80.65kN   112.08kN   144.57kN   169.86kN   181.97kN   212.42kN   225.11kN   241.09kN   271.97kN   280.68kN   
      33km/h   0.00kN   52.88kN   80.65kN   112.21kN   144.77kN   170.24kN   182.32kN   212.65kN   225.29kN   241.25kN   271.97kN   278.86kN   
      34km/h   0.00kN   52.88kN   80.81kN   112.33kN   144.96kN   170.61kN   182.67kN   212.87kN   225.47kN   241.41kN   271.97kN   277.05kN   
      35km/h   0.00kN   52.88kN   80.97kN   112.45kN   145.15kN   170.97kN   183.02kN   213.10kN   225.65kN   241.57kN   271.97kN   275.24kN   
      36km/h   0.00kN   52.88kN   81.12kN   112.58kN   145.35kN   171.34kN   183.36kN   213.32kN   225.83kN   241.73kN   271.97kN   273.42kN   
      37km/h   0.00kN   52.88kN   81.28kN   112.70kN   145.54kN   171.69kN   183.70kN   213.54kN   226.00kN   241.88kN   271.97kN   272.60kN   
      38km/h   0.00kN   53.09kN   81.44kN   112.82kN   145.73kN   172.05kN   184.04kN   213.76kN   226.18kN   242.04kN   271.01kN   270.64kN   
      39km/h   0.00kN   53.29kN   81.59kN   112.94kN   145.91kN   172.40kN   184.37kN   213.98kN   226.35kN   242.20kN   269.03kN   268.68kN   
      40km/h   0.00kN   53.49kN   81.75kN   113.06kN   146.10kN   172.74kN   184.70kN   214.20kN   226.53kN   242.36kN   267.06kN   266.72kN   
      41km/h   0.00kN   53.69kN   81.90kN   113.18kN   146.29kN   173.09kN   185.02kN   214.41kN   226.70kN   242.51kN   265.08kN   264.76kN   
      42km/h   0.00kN   53.89kN   82.06kN   113.30kN   146.47kN   173.43kN   185.35kN   214.63kN   226.87kN   242.67kN   263.11kN   262.80kN   
      43km/h   0.00kN   54.09kN   82.21kN   113.42kN   146.65kN   173.76kN   185.67kN   214.84kN   227.04kN   242.82kN   261.13kN   260.85kN   
      44km/h   0.00kN   54.28kN   82.36kN   113.54kN   146.84kN   174.09kN   185.98kN   215.05kN   227.22kN   242.98kN   259.16kN   258.89kN   
      45km/h   0.00kN   54.47kN   82.51kN   113.65kN   147.02kN   174.42kN   186.30kN   215.26kN   227.39kN   243.13kN   257.19kN   256.94kN   
      46km/h   0.00kN   54.66kN   82.66kN   113.77kN   147.20kN   174.75kN   186.61kN   215.32kN   227.55kN   243.28kN   255.22kN   254.99kN   
      47km/h   0.00kN   54.85kN   82.81kN   113.89kN   147.38kN   175.07kN   186.91kN   215.32kN   227.72kN   243.43kN   253.25kN   253.04kN   
      48km/h   0.00kN   55.04kN   82.95kN   114.00kN   147.55kN   175.39kN   187.22kN   215.32kN   227.89kN   243.59kN   251.28kN   251.09kN   
      49km/h   0.00kN   55.23kN   83.10kN   114.12kN   147.73kN   175.70kN   187.52kN   215.32kN   228.06kN   243.74kN   249.32kN   249.14kN   
      50km/h   0.00kN   55.41kN   83.25kN   114.23kN   147.91kN   176.01kN   187.82kN   215.32kN   228.22kN   243.89kN   247.35kN   247.19kN   
      51km/h   0.00kN   55.60kN   83.39kN   114.35kN   148.08kN   176.32kN   188.11kN   215.32kN   228.39kN   242.60kN   245.39kN   245.25kN   
      52km/h   0.00kN   55.78kN   83.54kN   114.46kN   148.25kN   176.63kN   188.41kN   215.32kN   228.55kN   240.98kN   243.55kN   243.43kN   
      53km/h   0.00kN   55.96kN   83.68kN   114.58kN   148.43kN   176.93kN   188.70kN   215.32kN   228.72kN   239.37kN   241.57kN   241.46kN   
      54km/h   0.00kN   56.14kN   83.82kN   114.69kN   148.60kN   177.23kN   188.98kN   215.32kN   228.88kN   237.76kN   239.59kN   239.50kN   
      55km/h   0.00kN   56.32kN   83.96kN   114.80kN   148.77kN   177.53kN   189.27kN   215.32kN   229.04kN   236.15kN   237.62kN   237.54kN   
      56km/h   0.00kN   56.49kN   84.10kN   114.91kN   148.94kN   177.82kN   189.55kN   215.32kN   229.21kN   234.54kN   235.64kN   235.59kN   
      57km/h   0.00kN   56.67kN   84.24kN   115.03kN   149.11kN   178.11kN   189.83kN   215.32kN   229.37kN   232.94kN   233.67kN   233.63kN   
      58km/h   0.00kN   56.84kN   84.38kN   115.14kN   149.27kN   178.40kN   190.11kN   215.32kN   229.53kN   231.33kN   231.70kN   231.68kN   
      59km/h   0.00kN   57.01kN   84.52kN   115.25kN   149.44kN   178.68kN   190.38kN   215.32kN   229.69kN   229.72kN   229.72kN   229.72kN   
      60km/h   0.00kN   57.18kN   84.66kN   115.36kN   149.61kN   175.44kN   186.98kN   214.30kN   225.65kN   227.69kN   229.72kN   229.72kN   
      61km/h   0.00kN   57.35kN   84.80kN   115.47kN   149.77kN   172.24kN   183.62kN   210.54kN   221.66kN   223.70kN   226.11kN   226.11kN   
      62km/h   0.00kN   57.52kN   84.93kN   115.58kN   149.93kN   169.08kN   180.29kN   206.82kN   217.70kN   219.75kN   222.17kN   222.17kN   
      63km/h   0.00kN   57.69kN   85.07kN   115.69kN   147.19kN   165.97kN   177.01kN   203.14kN   213.79kN   215.84kN   218.26kN   218.26kN   
      64km/h   0.00kN   57.85kN   85.20kN   115.80kN   144.50kN   162.93kN   173.78kN   199.51kN   209.93kN   211.97kN   214.39kN   214.39kN   
      65km/h   0.00kN   58.02kN   85.34kN   115.90kN   141.86kN   159.95kN   170.62kN   195.92kN   206.14kN   208.17kN   210.57kN   210.57kN   
      66km/h   0.00kN   58.18kN   85.47kN   116.01kN   139.29kN   157.04kN   167.53kN   192.40kN   202.42kN   204.43kN   206.81kN   206.81kN   
      67km/h   0.00kN   58.34kN   85.60kN   113.92kN   136.78kN   154.22kN   164.51kN   188.95kN   198.78kN   200.76kN   203.11kN   203.11kN   
      68km/h   0.00kN   58.50kN   85.74kN   111.90kN   134.35kN   151.49kN   161.58kN   185.58kN   195.23kN   197.17kN   199.49kN   199.49kN   
      69km/h   0.00kN   58.66kN   85.87kN   109.94kN   132.00kN   148.86kN   158.75kN   182.29kN   191.79kN   193.68kN   195.96kN   195.96kN   
      70km/h   0.00kN   58.82kN   86.00kN   108.05kN   129.74kN   146.32kN   156.01kN   179.10kN   188.44kN   190.29kN   192.51kN   192.51kN   
      71km/h   0.00kN   58.97kN   84.54kN   106.23kN   127.57kN   143.89kN   153.37kN   176.01kN   185.21kN   187.01kN   189.17kN   189.17kN   
      72km/h   0.00kN   59.13kN   83.15kN   104.48kN   125.48kN   141.56kN   150.84kN   173.03kN   182.10kN   183.84kN   185.93kN   185.93kN   
      73km/h   0.00kN   59.28kN   81.81kN   102.82kN   123.49kN   139.33kN   148.42kN   170.16kN   179.12kN   180.79kN   182.81kN   182.81kN   
      74km/h   0.00kN   59.43kN   80.54kN   101.22kN   121.59kN   137.21kN   146.11kN   167.40kN   176.25kN   177.86kN   179.80kN   179.80kN   
      75km/h   0.00kN   58.54kN   79.32kN   99.71kN   119.78kN   135.20kN   143.90kN   164.76kN   173.52kN   175.05kN   176.92kN   176.92kN   
      76km/h   0.00kN   57.68kN   78.17kN   98.27kN   118.06kN   133.29kN   141.81kN   162.23kN   170.91kN   172.37kN   174.15kN   174.15kN   
      77km/h   0.00kN   56.87kN   77.07kN   96.90kN   116.44kN   131.49kN   139.82kN   159.83kN   168.42kN   169.82kN   171.51kN   171.51kN   
      78km/h   0.00kN   56.10kN   76.03kN   95.61kN   114.90kN   129.78kN   137.93kN   157.54kN   166.07kN   167.38kN   168.99kN   168.99kN   
      79km/h   0.00kN   55.37kN   75.05kN   94.38kN   113.44kN   128.17kN   136.15kN   155.36kN   163.83kN   165.07kN   166.59kN   166.59kN   
      80km/h   0.00kN   54.69kN   74.13kN   93.23kN   112.07kN   126.66kN   134.47kN   153.30kN   161.71kN   162.88kN   164.31kN   164.31kN   
      81km/h   0.00kN   54.04kN   73.25kN   92.14kN   110.78kN   125.23kN   132.88kN   151.35kN   159.71kN   160.81kN   162.15kN   162.15kN   
      82km/h   0.00kN   53.43kN   72.43kN   91.12kN   109.56kN   123.88kN   131.39kN   149.50kN   157.82kN   158.85kN   160.11kN   160.11kN   
      83km/h   0.00kN   52.85kN   71.65kN   90.16kN   108.42kN   122.62kN   129.98kN   147.76kN   156.04kN   156.99kN   158.17kN   158.17kN   
      84km/h   0.00kN   52.31kN   70.92kN   89.25kN   107.35kN   121.44kN   128.66kN   146.11kN   154.36kN   155.25kN   156.34kN   156.34kN   
      85km/h   0.00kN   51.80kN   70.24kN   88.40kN   106.34kN   120.32kN   127.41kN   144.57kN   152.78kN   153.60kN   154.61kN   154.61kN   
      86km/h   0.00kN   51.32kN   69.59kN   87.60kN   105.39kN   119.28kN   126.25kN   143.11kN   151.29kN   152.05kN   152.99kN   152.99kN   
      87km/h   0.00kN   50.88kN   68.99kN   86.85kN   104.50kN   118.30kN   125.15kN   141.73kN   149.89kN   150.59kN   151.45kN   151.45kN   
      88km/h   0.00kN   50.46kN   68.42kN   86.15kN   103.67kN   117.39kN   124.12kN   140.44kN   148.58kN   149.22kN   150.01kN   150.01kN   
      89km/h   0.00kN   50.06kN   67.89kN   85.49kN   102.89kN   116.53kN   123.16kN   139.23kN   147.35kN   147.93kN   148.65kN   148.65kN   
      90km/h   0.00kN   49.69kN   67.39kN   84.87kN   102.16kN   115.72kN   122.25kN   138.08kN   146.19kN   146.71kN   147.37kN   147.37kN   
      91km/h   0.00kN   49.34kN   66.93kN   84.29kN   101.47kN   114.97kN   121.40kN   137.01kN   145.10kN   145.58kN   146.17kN   146.17kN   
      92km/h   0.00kN   49.02kN   66.49kN   83.75kN   100.83kN   114.27kN   120.61kN   136.01kN   144.08kN   144.51kN   145.04kN   145.04kN   
      93km/h   0.00kN   48.71kN   66.08kN   83.24kN   100.23kN   113.61kN   119.86kN   135.06kN   143.12kN   143.50kN   143.97kN   143.97kN   
      94km/h   0.00kN   48.43kN   65.69kN   82.76kN   99.66kN   112.99kN   119.16kN   134.17kN   142.22kN   142.56kN   142.98kN   142.98kN   
      95km/h   0.00kN   48.16kN   65.33kN   82.32kN   99.13kN   112.41kN   118.51kN   133.34kN   141.38kN   141.67kN   142.04kN   142.04kN   
      96km/h   0.00kN   47.91kN   64.99kN   81.90kN   98.64kN   111.86kN   117.89kN   132.56kN   140.59kN   140.84kN   141.16kN   141.16kN   
      97km/h   0.00kN   47.67kN   64.67kN   81.50kN   98.17kN   111.35kN   117.32kN   131.82kN   139.85kN   140.06kN   140.33kN   140.33kN   
      98km/h   0.00kN   47.45kN   64.38kN   81.13kN   97.74kN   110.88kN   116.78kN   131.13kN   139.15kN   139.33kN   139.55kN   139.55kN   
      99km/h   0.00kN   47.24kN   64.10kN   80.79kN   97.33kN   110.43kN   116.27kN   130.48kN   138.49kN   138.64kN   138.82kN   138.82kN   
      100km/h   0.00kN   47.05kN   63.83kN   80.46kN   96.95kN   110.01kN   115.80kN   129.88kN   137.88kN   137.99kN   138.13kN   138.13kN   
      101km/h   0.00kN   46.87kN   63.59kN   80.16kN   96.59kN   109.62kN   115.35kN   129.30kN   137.30kN   137.39kN   137.49kN   137.49kN   
      102km/h   0.00kN   46.70kN   63.36kN   79.88kN   96.25kN   109.25kN   114.93kN   128.77kN   136.76kN   136.82kN   136.88kN   136.88kN   
      103km/h   0.00kN   46.53kN   63.14kN   79.61kN   95.93kN   108.90kN   114.54kN   128.26kN   136.25kN   136.28kN   136.31kN   136.31kN   
      104km/h   0.00kN   46.38kN   62.94kN   79.36kN   95.64kN   108.57kN   114.17kN   127.79kN   135.78kN   135.78kN   135.78kN   135.78kN   
      105km/h   0.00kN   46.09kN   62.54kN   78.86kN   95.04kN   107.89kN   113.45kN   126.99kN   133.59kN   133.59kN   133.59kN   133.59kN   
      106km/h   0.00kN   45.80kN   62.14kN   78.35kN   94.43kN   107.20kN   112.73kN   126.18kN   131.41kN   131.41kN   131.41kN   131.41kN   
      107km/h   0.00kN   45.50kN   61.74kN   77.85kN   93.82kN   106.51kN   112.00kN   125.36kN   129.24kN   129.24kN   129.24kN   129.24kN   
      108km/h   0.00kN   45.20kN   61.33kN   77.33kN   93.20kN   105.81kN   111.26kN   124.53kN   127.09kN   127.09kN   127.09kN   127.09kN
      109km/h   0.00kN   44.90kN   60.92kN   76.81kN   92.57kN   105.10kN   110.51kN   123.70kN   124.94kN   124.94kN   124.94kN   124.94kN   
      110km/h   0.00kN   44.59kN   60.51kN   76.29kN   91.94kN   104.38kN   109.76kN   122.86kN   122.86kN   122.86kN   122.86kN   122.86kN   
      111km/h   0.00kN   44.28kN   60.09kN   75.76kN   91.31kN   103.66kN   109.00kN   120.72kN   120.72kN   120.72kN   120.72kN   120.72kN   
      112km/h   0.00kN   43.97kN   59.67kN   75.23kN   90.66kN   102.93kN   108.23kN   118.58kN   118.58kN   118.58kN   118.58kN   118.58kN   
      113km/h   0.00kN   43.66kN   59.24kN   74.69kN   90.01kN   102.19kN   107.46kN   116.46kN   116.46kN   116.46kN   116.46kN   116.46kN   
      114km/h   0.00kN   43.34kN   58.81kN   74.15kN   89.36kN   101.45kN   106.67kN   114.35kN   114.35kN   114.35kN   114.35kN   114.35kN   
      115km/h   0.00kN   43.02kN   58.37kN   73.60kN   88.70kN   100.69kN   105.88kN   112.25kN   112.25kN   112.25kN   112.25kN   112.25kN   
      116km/h   0.00kN   42.69kN   57.93kN   73.04kN   88.03kN   99.94kN   105.08kN   110.15kN   110.15kN   110.15kN   110.15kN   110.15kN   
      117km/h   0.00kN   42.37kN   57.49kN   72.48kN   87.35kN   99.17kN   104.28kN   108.07kN   108.07kN   108.07kN   108.07kN   108.07kN   
      118km/h   0.00kN   42.03kN   57.04kN   71.92kN   86.67kN   98.39kN   103.46kN   106.00kN   106.00kN   106.00kN   106.00kN   106.00kN   
      119km/h   0.00kN   41.70kN   56.58kN   71.34kN   85.98kN   97.61kN   102.64kN   103.95kN   103.95kN   103.95kN   103.95kN   103.95kN   
      120km/h   0.00kN   41.36kN   56.13kN   70.77kN   85.29kN   96.82kN   101.81kN   101.90kN   101.90kN   101.90kN   101.90kN   101.90kN   
      121km/h   0.00kN   41.02kN   55.66kN   70.18kN   84.58kN   96.02kN   99.87kN   99.87kN   99.87kN   99.87kN   99.87kN   99.87kN   
      122km/h   0.00kN   40.68kN   55.20kN   69.59kN   83.87kN   95.22kN   97.90kN   97.90kN   97.90kN   97.90kN   97.90kN   97.90kN   
      123km/h   0.00kN   40.33kN   54.72kN   69.00kN   83.16kN   94.41kN   95.88kN   95.88kN   95.88kN   95.88kN   95.88kN   95.88kN   
      124km/h   0.00kN   39.98kN   54.25kN   68.40kN   82.43kN   93.58kN   93.87kN   93.87kN   93.87kN   93.87kN   93.87kN   93.87kN   
      125km/h   0.00kN   39.63kN   53.77kN   67.79kN   81.70kN   91.87kN   91.87kN   91.87kN   91.87kN   91.87kN   91.87kN   91.87kN   
      126km/h   0.00kN   39.27kN   53.28kN   67.18kN   80.97kN   89.89kN   89.89kN   89.89kN   89.89kN   89.89kN   89.89kN   89.89kN   
      127km/h   0.00kN   38.91kN   52.79kN   66.56kN   80.22kN   87.93kN   87.93kN   87.93kN   87.93kN   87.93kN   87.93kN   87.93kN   
      128km/h   0.00kN   38.54kN   52.30kN   65.94kN   79.47kN   86.06kN   86.06kN   86.06kN   86.06kN   86.06kN   86.06kN   86.06kN   
      129km/h   0.00kN   38.17kN   51.80kN   65.31kN   78.71kN   84.11kN   84.11kN   84.11kN   84.11kN   84.11kN   84.11kN   84.11kN   
      130km/h   0.00kN   37.80kN   51.29kN   64.67kN   77.94kN   82.16kN   82.16kN   82.16kN   82.16kN   82.16kN   82.16kN   82.16kN   
      131km/h   0.00kN   37.43kN   50.78kN   64.03kN   77.17kN   80.24kN   80.24kN   80.24kN   80.24kN   80.24kN   80.24kN   80.24kN   
      132km/h   0.00kN   37.05kN   50.27kN   63.38kN   76.39kN   78.33kN   78.33kN   78.33kN   78.33kN   78.33kN   78.33kN   78.33kN   
      133km/h   0.00kN   36.66kN   49.75kN   62.73kN   75.60kN   76.43kN   76.43kN   76.43kN   76.43kN   76.43kN   76.43kN   76.43kN   
      134km/h   0.00kN   36.28kN   49.23kN   62.07kN   74.55kN   74.55kN   74.55kN   74.55kN   74.55kN   74.55kN   74.55kN   74.55kN   
      135km/h   0.00kN   35.89kN   48.70kN   61.40kN   72.69kN   72.69kN   72.69kN   72.69kN   72.69kN   72.69kN   72.69kN   72.69kN   
      136km/h   0.00kN   35.50kN   48.16kN   60.73kN   70.84kN   70.84kN   70.84kN   70.84kN   70.84kN   70.84kN   70.84kN   70.84kN   
      137km/h   0.00kN   35.10kN   47.62kN   60.05kN   69.01kN   69.01kN   69.01kN   69.01kN   69.01kN   69.01kN   69.01kN   69.01kN   
      138km/h   0.00kN   34.70kN   47.08kN   59.36kN   67.20kN   67.20kN   67.20kN   67.20kN   67.20kN   67.20kN   67.20kN   67.20kN   
      139km/h   0.00kN   34.29kN   46.53kN   58.67kN   65.40kN   65.40kN   65.40kN   65.40kN   65.40kN   65.40kN   65.40kN   65.40kN   
      140km/h   0.00kN   33.88kN   45.98kN   57.97kN   63.69kN   63.69kN   63.69kN   63.69kN   63.69kN   63.69kN   63.69kN   63.69kN   
   )                                          
)
        
comment (**vnitrni zvuk **)

        Sound ( "..\\..\\common.snd\\sndX6X\\363cab-IH-OR.sms" )
        
comment (** pohled z kabiny **)

	CabView ( "..\\..\\common.cab\\cab362\\363-OR.cvf" )
	
comment (** vnejsi pohled z okna - klavesa "HOME" **)

	HeadOut ( 1.65 3.0 6.6 )

comment (** brzdy - brzdove systemy a ovladaci prvky **)
	
	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
  	BrakesEngineControllers( "Independent, Train, Dynamic, Blended" )

comment (** kompresor a tlaky v jimkach, vlastnosti potrubi **)

	AirBrakesMainMaxAirPressure( 10bar )
	AirBrakesCompressorRestartPressure( 8.5bar )
	AirBrakesMainResVolume( 900l )
	comment (** doba plneni hlavni jimky/vykon kompresoru - vypoctena doba plneni 900l jimky 4.48min.
  	  	kompresor SKE 180L, prikon 15kW, saci vykon 120m^3/h. Vypoctena rychlost plneni jimky 0.04bar/s**)
	ORTSMainResChargingRate ( 0.04bar/s )
	ORTSBrakePipeChargingRate ( 4.6bar/s )
	AirBrakesAirCompressorWattage( 15000 )
	AirBrakesIsCompressorElectricOrMechanical( 0 )
	comment (** unik vzduchu netesnosti brzdoveho potrubi **)
	TrainPipeLeakRate ( 0.00066bar/s )
	ORTSBrakePipeTimeFactor ( 0.003 )
	ORTSBrakeServiceTimeFactor ( 1.009 )
	ORTSBrakeEmergencyTimeFactor ( 0.1 )

comment (** samocinna prubezna brzda - brzdic DAKO BSE **)

	TrainBrakesControllerMaxSystemPressure ( 5bar )
	TrainBrakesControllerMaxQuickReleaseRate ( 1.92bar/s )
	TrainBrakesControllerMaxReleaseRate ( 0.215bar/s )
	TrainBrakesControllerMaxApplicationRate ( 0.215bar/s )
	TrainBrakesControllerEmergencyApplicationRate ( 2.35bar/s )
	TrainBrakesControllerFullServicePressureDrop ( 1.5bar )
	TrainBrakesControllerMinPressureReduction ( 0.2bar )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )

comment (** primocinna brzda DAKO BP **)

	EngineBrakesControllerMaxSystemPressure ( 5bar )
	EngineBrakesControllerMaxReleaseRate ( 1.4bar/s )
	EngineBrakesControllerMaxApplicationRate (1.4bar/s )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerEmergencyApplicationRate ( 0.159bar/s )
	EngineBrakesControllerFullServicePressureDrop ( 1.5bar )
	EngineBrakesControllerMinPressureReduction ( 0.2bar )
	EngineBrakesControllerEmergencyBrakeTimePenalty ( 0 )
  	EngineBrakesControllerHasProportionalBrake ( 1 )
  	EngineBrakesProportionalBrakeLag ( 0 )


comment (** EDB **)
	DynamicBrakesMaximumForce		( 160kN )
	DynamicBrakesResistorCurrentLimit	( 715 )
	DynamicBrakesDelayTimeBeforeEngaging	( 0 )
	DynamicBrakesNumberOfControllerNotches	( 20 )
	DynamicBrakesMaxAirBrakePressure	( 3.5bar )
	DynamicBrakeHasAutoBailOff		( 1 )
	ORTSDynamicBlendingForceMatch ( 0 )
        ORTSDynamicBlendingOverride ( 0 )


comment (** krivky prubehu brzdne sily EDB - autor: Igor Hnizdo **)

        ORTSDynamicBrakeForceCurves (

               0.00 (
                    0km/h    0kN
                    120km/h  0kN
               )

               1.00 (
                    0km/h    0kN
                    2km/h    0kN
                    4km/h    3kN
                    5km/h    10kN
                    6km/h    38kN
                    7km/h    40kN
                    10km/h   55kN
                    28km/h   160kN
                    68km/h   160kN
                    70km/h   156kN
                    77km/h   140kN
                    80km/h   136kN
                    90km/h   120kN
                    100km/h  108kN
                    110km/h  98kN
                    120km/h  89kN
               )

        )


comment (** bezpecnostni monitory **)


comment (** "zivak" **)
	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 16 )
		MonitoringDeviceAlarmTimeLimit ( 6 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)

 Comment	(** Ovladaci prvky **)

	EngineControllers (

		comment (** ovladani vykonu **)
		Throttle ( 0 1 0.02 0
			NumNotches ( 1
				Notch( 0 1 Dummy )
			)
                )


		Comment (** Brzdic Dako BP **)
		Brake_Engine ( 0 1 0.04 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)


        Comment (** Brzdic Dako BSE **)
		Brake_Train 	( 0 1 0.1 0.6
			     NumNotches ( 6
				
				Notch ( 0.0 0 TrainBrakesControllerFullQuickReleaseStart )
				Notch ( 0.2 0 TrainBrakesControllerHoldLappedStart )
				Notch ( 0.4 0 TrainBrakesControllerReleaseStart )
				Notch ( 0.6 0 TrainBrakesControllerNeutralHandleOffStart )
				Notch ( 0.8 0 TrainBrakesControllerApplyStart )
				Notch ( 0.95 0 TrainBrakesControllerEmergencyStart )
			     )
                )

	Comment (** EDB **)
		  Brake_Dynamic ( 0 1 0.05 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)

       	    comment (** rucni brzda **)
		Brake_Hand 	( 0 1 0.1 0
			NumNotches ( 0 )
		)

                AWS ( 0 1 0 )
		BailOffButton 	( 0 1 0 )
		BellToggle 	( 0 1 0 )
		DirControl 		( -1 0 1 1 )
		EmergencyStopToggle	( 0 1 0 )
		Headlights 		( 0 0.5 1 0 )
		Horn 			( 0 1 0 )
		PantographsToggle_4 ( 0 1 0 )
		Sanding 		( 0 1 0 )
		Vigilance 		( 0 1 0 )
		Wipers 			( 0 1 0 )
	)

comment (** nazev stroje v menu ORTS **)
	Name ( "CD 363.001-9 HK -ORTS" )

comment (** popis **)
	Description (
		"Rada 363 CD je univerzalni elektricka skrinova lokomotiva, pouzivana v osobni a nákladní doprave.\nTyp Bo'-Bo', napeti 3kV ss , 25kV 50Hz str.\n\nDelka pres narazniky: 16,8 m\n\nPrumer hnacich kol: 1250 mm\n\nHmotnost ve sluzbe: 87 t\n\n" +
		"Trvaly vykon trakcnich motoru: 3480 kW ss , 3060kW str.\n\n" +
		"Max. rychlost 120 km/h\n" +
		""
	)
)